// 2.4L Datsun stright six IMSA GTU, GR-4 race engine. V1.5
RPMTorque=( 0.0, -58.4, -58.0)
RPMTorque=( 250.0, -33.0, -9.0)
RPMTorque=( 500.0, -13.7, 60.0)
RPMTorque=( 750.0, -22.0, 120.0)
RPMTorque=( 1000.0, -30.4, 168.3)
RPMTorque=( 1250.0, -35.0, 186.1)
RPMTorque=( 1500.0, -40.0, 195.0)
RPMTorque=( 1750.0, -25.0, 202.2)
RPMTorque=( 2000.0, -49.6, 209.3)
RPMTorque=( 2250.0, -53.0, 217.3)
RPMTorque=( 2500.0, -55.2, 224.4)
RPMTorque=( 2750.0, -60.0, 230.7)
RPMTorque=( 3000.0, -65.2, 239.6)
RPMTorque=( 3250.0, -71.0, 246.7)
RPMTorque=( 3500.0, -78.7, 254.7)
RPMTorque=( 3750.0, -85.0, 262.7)
RPMTorque=( 4000.0, -92.0, 267.2)
RPMTorque=( 4250.0, -98.0, 274.3)
RPMTorque=( 4500.0, -105.9, 280.5)
RPMTorque=( 4750.0, -110.9, 284.1)
RPMTorque=( 5000.0, -120.1, 286.8)
RPMTorque=( 5250.0, -133.0, 290.3)
RPMTorque=( 5500.0, -145.6, 292.1)
RPMTorque=( 5750.0, -157.0, 293.9)
RPMTorque=( 6000.0, -169.5, 294.0)
RPMTorque=( 6250.0, -176.0, 293.0)
RPMTorque=( 6500.0, -184.7, 289.0)
RPMTorque=( 6750.0, -193.0, 283.0)
RPMTorque=( 7000.0, -200.2, 275.0)
RPMTorque=( 7250.0, -213.0, 267.2)
RPMTorque=( 7500.0, -226.0, 261.0)
RPMTorque=( 7750.0, -238.0, 254.7)
RPMTorque=( 8000.0, -252.2, 249.0)
RPMTorque=( 8250.0, -275.0, 242.0)
RPMTorque=( 8500.0, -298.8, 230.0)
RPMTorque=( 8750.0, -315.0, 207.5)
RPMTorque=( 9000.0, -326.8, 185.2)
RPMTorque=( 9250.0, -334.2, 147.8)
RPMTorque=( 9500.0, -344.7, 83.7)
RPMTorque=( 9750.0, -352.3, 10.0)
FuelConsumption=3.000e-05   // affected by throttle position and engine speed
FuelEstimate=1.20   // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.18000   // rotational inertia of engine components
IdleThrottle=1   // throttle multiplier to help maintain idle speed
IdleRPMLogic=(1050, 1250)   // attempt to maintain idle speed between these RPMs
LaunchEfficiency=0.50000   // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(6000, 7000)   // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(8300, 100, 1)   
RevLimitSetting=0   
RevLimitLogic=150   // RPM range around current setting where rev limiter operates
RevLimitAvailable=1   // whether to use a rev limit (if 0, you still must have a "rev limit", just make it 40000 or so, and make sure to change [CONTROLS]->UpshiftAlgorithm to fix shifting points)
EngineMapRange=(0, 1, 5)   // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=2   
EngineBrakingMapRange=(0, 7.700e-04, 10)   // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=4   // the default is 1 * 0.000133 * 15000 RPM = 2% applied throttle at zero input throttle
EngineBoostRange=(0.01000, 1, 10)   
EngineBoostSetting=1   
BoostEffects=(15, 0.0100, 1)   // RPM increase per setting, fuel increase (1%) per setting, engine wear rate (101.5%) per setting
BoostTorque=-0.00410   // 0.4% less torque per setting (applies to all RPMs)
BoostPower=1.600e-04   // % more horsepower per setting
OptimumOilTemp=95   // degrees Celsius at which engine operates optimally
CombustionHeat=40   // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=0.00120   // heat added linearly with engine speed
OilMinimumCooling=0.00750   // heat dissipated without oil/water transfer
OilWaterHeatTransfer=(0.39620, 7.925e-05)   // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=0.00396   // heat dissipated without radiator
RadiatorCooling=(1.592e-04, 1.004e-04)   // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=(7900, 95)   // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(100, 3)   // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=10800   // average lifetime in seconds
LifetimeVar=2250   // lifetime random variance
EngineEmission=(0, 0.6000, -2.6000)   // where flames and smoke are emitted (relative to ref frame at rear axle)
EngineSound=(0, 0.5000, -2.4000)   // where engine sound is played (relative to ref frame at rear axle)
SpeedLimiter=1   // whether vehicle has a pitlane speed limiter
OnboardStarter=1   // whether vehicle restarts when stalled
StarterTiming=(1, 0.0, 0.4000)   // average and variable cranking time, then time to blend with starting sound
